|  |  |  |  |
| --- | --- | --- | --- |
| System Name | Brookings | PWS ID# | 4 1 00149 |
| Month/Year  | 01/2024 | Entry Point: | A | Required Minimum Residual : | Variable – see column headers |
| Date | Time | Source(s) in use | Lowest free chlorine residual at WTP influent (minimum 0.1 mg/L) | In emergency, when influent not met – use filter trains & monitor at Entry Pt(minimum 0.3 mg/L) | Notes |
| 1 | 2230 | SRC-AA | .39 |  |  |
| 2 | 0528 | SRC-AA | .39 |  |  |
| 3 | 1356 | SRC-AA | .41 |  |  |
| 4 | 1912 | SRC-AA | .38 |  |  |
| 5 | 1843 | SRC-AA | .38 |  |  |
| 6 | 1215 | SRC-AA | .34 |  |  |
| 7 | 1925 | SRC-AA | .39 |  |  |
| 8 | 0800 | SRC-AA | .36 |  |  |
| 9 | 0752 | SRC-AA | .32 |  |  |
| 10 | 1030 | SRC-AA | .25 |  |  |
| 11 | 0101 | SRC-AA | .36 |  |  |
| 12 | 1732 | SRC-AA | .37 |  |  |
| 13 | 0917 | SRC-AA | .29 |  |  |
| 14 | 0940 | SRC-AA | .26 |  |  |
| 15 | 0540 | SRC-AA | .37 |  |  |
| 16 | 0810 | SRC-AA | .35 |  |  |
| 17 | 1419 | SRC-AA | .29 |  |  |
| 18 | 1538 | SRC-AA | .32 |  |  |
| 19 | 1614 | SRC-AA | .32 |  |  |
| 20 | 0328 | SRC-AA | .28 |  |  |
| 21 | 1850 | SRC-AA | .32 |  |  |
| 22 | 0715 | SRC-AA | .36 |  |  |
| 23 | 0200 | SRC-AA | .34 |  |  |
| 24 | 0309 | SRC-AA | .32 |  |  |
| 25 | 1816 | SRC-AA | .31 |  |  |
| 26 | 0314 | SRC-AA | .33 |  |  |
| 27 | 2015 | SRC-AA | .33 |  |  |
| 28 | 0340 | SRC-AA | .33 |  |  |
| 29 | 1940 | SRC-AA | .34 |  |  |
| 30 | 0452 | SRC-AA | .34 |  |  |
| 31 | 0442 | SRC-AA | .33 |  |  |
| Was the chlorine residual ever less than the required minimum residual of 0.1 mg/L? [ ] Yes [x] NoIf yes, what was the longest time period until the required level was restored?  |
| **GWS Serving 3,300 or Fewer** | **GWS Serving More Than 3,300** |
| If yes, did you monitor every four hours until the residual returned to       mg/L as required? [ ] Yes [ ] No *Attach those results and submit them with this form.* | Did continuous monitoring equipment fail at any time this reporting month? [ ]  Yes [x] NoIf yes, were grab samples collected every four hours until the continuous monitoring equipment was returned to service as required? [ ] Yes [ ]  No required since it was less than 4 hours.  | Date continuous monitoring equipment failed:      /       /      Date it was returned to service:       /       /       |
| Printed Name: Jeff A. Houchin | Title: Area Manager - Jacobs  | Operator Certification #:6497  |
| Signature: C:\Documents and Settings\jhouchi1\My Documents\Mail\OL Temp Attachments\Houchin_Jeff_OMI00023245.gif | Phone #: 503-313-5808 | OR |
| Date: 2 / 7 / 2024 |  | Small Groundwater System [x]  |

***Return by 10th of following month by either email*** ***dwp.dmce@state.or.us******; fax 971-673-0694;***
***or mail to Drinking Water Services, PO Box 14350, Portland, OR 97293-0350.***

***August 22, 2019***