Water Quality Parameter Monitoring Form

**Lead & Copper Rule Corrosion Control**

<<Have minimums been met for this day?

**ENTRY POINT**

**PWS ID: 41**

**System Name: Bay City Water System**

**Entry Point: Wells Sample Period: 05/2023**

*Month/Year*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Day** | **pH** | **Alk** | **Phos** | **Other** | **Y/N** |
| 1 | 7.7 |  |  |  |  |
| 2 | 7.7 |  |  |  |  |
| 3 | 7.7 |  |  |  |  |
| 4 | 7.7 |  |  |  |  |
| 5 | 7.7 |  |  |  |  |
| 6 | 7.6 |  |  |  |  |
| 7 | 7.7 |  |  |  |  |
| 8 | 7.7 |  |  |  |  |
| 9 | 7.7 |  |  |  |  |
| 10 | 7.7 |  |  |  |  |
| 11 | 7.77.7 |  |  |  |  |
| 12 | 7.7 |  |  |  |  |
| 13 | 7.6 |  |  |  |  |
| 14 | 7.6 |  |  |  |  |
| 15 | 7.6 |  |  |  |  |
| 16 | 7.6 |  |  |  |  |
| 17 | 7.6 |  |  |  |  |
| 18 | 7.6 |  |  |  |  |
| 19 | 7.6 |  |  |  |  |
| 20 | 7.6 |  |  |  |  |
| 21 | 7.6 |  |  |  |  |
| 22 | 7.6 |  |  |  |  |
| 23 | 7.6 |  |  |  |  |
| 24 | 7.6 |  |  |  |  |
| 25 | 7.6 |  |  |  |  |
| 26 | 7.6 |  |  |  |  |
| 27 | 7.6 |  |  |  |  |
| 28 | 7.6 |  |  |  |  |
| 29 | 7.6 |  |  |  |  |
| 30 | 7.6 |  |  |  |  |
| 31 | 7.6 |  |  |  |  |
|  |  |  0 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **0** | **0** | **0** | **7** | **9** |

**Number of excursions\* during this month: 0** *(Count the number of days when any WQP was less than the minimum required)*

**Total excursions during the previous 5 months: 0** *(Over 9 excursions in 6 months is a violation. Entry Point and Distribution excursions are cumulative )*

*For OHA use only*

# Minimum Water Quality Parameters as set by

pH

|  |
| --- |
| **7.4** |
|  |
|  |
|  |

Alk PO4

Other

*(Alkalinity) (Orthophosphate) ( )*

(No = N = Excursion)

**Total N's**

# Print Name: Brian Bettis Signature: Date: 06/06/2023

Send to DWP within 10 days after end of sampling period

OHA Drinking Water Program, PO Box 14350, Portland, OR 97293-0350 Phone (971) 673-0405 Website: <http://healthoregon.org/dwp/>